## Definition Modes

The definition modes use a simple "define by selection" mechanism to construct new elements. You choose a certain definition mode by clicking on its icon in the toolbar. Then you are asked to select a certain number of elements in the view. After a sufficient number of elements are selected, the newly defined element is added to the construction. Although these modes are slightly inconvenient compared to the interactive modes, using these modes is sometimes unavoidable. There are four major circumstances in which the definition modes should be used:

- A certain geometric operation is provided only as a definition mode. (This is the case for the following modes: angle bisector, compass, circle by three points, center, conic by five points, polar of a point, polar of a line, and polygon.
- A point of intersection cannot not be reached in the visible area of a view. For instance, two lines can be almost parallel, so that their point of intersection lis far outside the viewing region in the window. Then the usual "add a point" or "add a line" modes are not applicable. But you can still select the lines and apply "meet" mode.
- An element could be invisible or complex. It can still be selected (e.g., in a "construction text" view), and a definition mode can be used.
- A situation could be ambiguous, such as three lines passing through a point. Then the interactive "add point" mode cannot be used to add a point of intersection (since all three lines would be close to the mouse pointer position). In this case, use "meet" mode and select the lines whose intersection is desired. In the case of a geometric theorem in which three lines always meet, such as the altitudes of a triangle, Cinderella's theorem checking mechanism ensures that the added point is considered incident to all three lines.

The definition modes are

| Center
| Angle Bisector
| Compass
| Mirror
| Circle by Three Points
| Conic by Five Points
| Ellipse by Foci
| Parabola by Focus and Directrix
| Hyperbola by Foci
| Polar of a Point
| Polar of a Line
| Polygon
| Intersection
| Arc
| Angle Mark

A few things are common to all definition modes and should be known in advance:

- Elements are selected by clicking them with the mouse pointer. The selection can be made in any of the geometric views, in particular in the construction text?, where all elements are always visible and selectable).
- Selected elements are highlighted in the view.
- Preselected elements are often considered when a definition mode is chosen. So if two lines are selected and you press the button that chooses "meet" mode, then the point of intersection is instantly added.
- If you made a mistake in selecting an element you can deselect it with a second click.
- You can also select the elements by moving the mouse while holding the mouse button down. All elements that are touched by the mouse pointer will be selected (or deselected).
- Selected elements that do not contribute to the required selection of the mode are ignored. For instance, if you choose circle by three points mode, all selected lines, circles, and conics are ignored.
- Selection modes communicate with the user using the message line. There you can find messages that tell you about the next expected input.

### See also

In addition to the standard modes that are provided with a button, there are also many new modes in Cinderella.2 that are accessible only via the menu. For these please consult the sections Polygons, Conic Operations, and Transformation Modes.

Page last modified on Tuesday 23 of May, 2006 [11:31:39 UTC].
The original document is available at http://doc.cinderella.de/tiki-index.php?page=Definition%20Modes